**2 Post Lift**

**1 SAFETY AND OPERATING INSTRUCTIONS**

1. When using this lift, basic safety precautions should always be followed, including the following.
2. Read all instructions in this manual and on the lift.
3. Inspect lift daily. Do not operate if it malfunctions or problems have been

encountered.

1. Never attempt to overload the lift. The manufacturer’s rated capacity is shown on

the identification label on the power side column. Do not override the operating

controls or the warranty will be void.

1. Before driving vehicle between the towers, position the arms to the drive-through

position to ensure unobstructed clearance. Do not hit or run over arms as this

could damage the lift and/or vehicle.

1. Only trained and authorized personnel should operate the lift. Do not allow

customers or bystanders to operate the lift or be in the lift area.

1. Position the lift support pads to contact the vehicle manufacturers recommended

lifting points. Raise the lift until the pads contact the vehicle. Check pads for secure contact with the vehicle. Check all arm restraints and insure they are properly engaged. Raise the lift to the desired working height.

1. Some pickup trucks may require an optional truck adapter to clear running boards or other accessories.

**NOTE:** Always use all 4 arms to raise and support vehicle.

1. **Caution! Never work under the lift unless the mechanical safety locks are**

**engaged.**

1. Note that the removal or installation of some vehicle parts may cause a critical load shift in the center of gravity and may cause the vehicle to become unstable. Refer to the vehicle manufacturer’s service manual for recommended procedures.
2. Always keep the lift area free of obstruction and debris. Grease and oil spills should always be cleaned up immediately.
3. Never raise vehicle with passengers inside.
4. Before lowering check area for any obstructions.
5. Before removing the vehicle from the lift area, position the arms to the drive- through position to prevent damage to the lift and /or vehicle.

**Scissor Lift**

**Safety Maintenance Bar Procedure**

**WARNING!!!**

ALWAYS use the safety bars for any service or maintenance. NEVER go under or reach under the lift unless both safety bars are securely in place and the power to the unit has been disconnected to prevent others from operating the lift. NEVER use the safety bars with a load on the platform.

**CAUTION**

Never use the lift unless the safety bars are properly stored or damage may occur to the equipment.

1. Remove the safety bars from their storage position.
2. Raise the lift to full travel, and place the safety bar. Make sure the safety bar

is in place.

1. Once BOTH safety bars are in place, slowly lower the lift until the safety bars

rest against the end of the baseframe. Visually inspect both safety

bars to insure they are secure.

1. To disengage the safety bars raise the lift to move the safety bars and make

sure lift operates correctly. Store the safety bars in the original position.